# Changes implemented on LED life-3 (rev-c)

1. Value of resistor in the LED path changed to 82 Ohms
2. Temperature sensor added to LED board
3. Connected the CLK pins of IO expanders for synchronization
4. Changed the reset of LED board to an independent reset from TIVA