# Changes implemented on Debug life-3 (rev-c)

1. JTAG connector added for Intel Debugging.
2. Connection changes to resolve the Intel Debug UART inversion is implemented
3. Two Level translators from GBC board have been moved to Debug board based on review feedback in SG
4. Debug Connector Orientation has been changed as per recommendation in review feedback in SG